Phillip May

Lab 1

Advanced microcontroller programming controllers\

**Part 1: Explorer 16 development board tour**

 Identify the ports for all user LEDS: Port A

 Identify the ports for user PBs S3 to S6: Rd6, RD13 and RA7

 Identify the Primary Oscillator crystal frequency: 8Mhz

**Part 3: Bits and bit fields**

At RA6 and measure the frequency and period: The frequency was 8Mhz

